**ПРИЛОЖЕНИЕ F  
(справочное)**

**Библиография**

[1] 89\392\ЕЕС: Council Directive of 14 June 1989 on the approximation of the laws of the Member States relating to machinery, amended by Directive 1\368\EEC

[2] A. R. Moritz, F. C. Henriques: The relative Importance of Time and Surface Temperature in the Causation of Cutaneous Bums. Studies of Thermal Injury II, Am. J. Path., Vol. 23, 1947, p. 659

[3] Y. С. Wu: Material Properties Criteria for Thermal Safety. Journal of Materials, Vol. 7, No. 4, p. 573, 1972

[4] Y. С. Wu: Control of Thermal Impact for Thermal Safety. AIAA Journal, Vol. 15, No. 5, p. 674, May 1977, American Institute of Aeronautics and Astronautics

[5] L. A. Marzetta: A Tecrmesthesiometer - An Instrument for Bum Hazard Measurement. IEEE Transactions on biomedical Engineering, Communications, September 1974

and L. A. Marzetta; Engineering and Construction Manual/or an Instrument to Make Bum Hazard Measurement in Consumer Products. NBS Technical Note 816 U.S. Department of Commerce National Bureau of Standards

[6] H. Siekmann: Bestimmung maximal tolerierbarer Temperaturen bei der Benihrung heifSer Oberflachen. Die BG (1983) Nr. 10, S. 525-530

and H. Siekmann: Determination of maximum temperatures that can be tolerated on contact with hot surfaces, Applied Ergonomics 1989, 20, 4, p. 313-317

[7] H. Siekmann: Empfohlene Maximaltemperaturen benihrbarer Oberflachen. Die BG (1986) Nr 8, 5, p. 436-438

and H. Siekmann; Recommended maximum temperatures for touchable surfaces, Applied Ergonomics 1990, 21, 4, 69-73

[8] H. Manzinger Temperaturgremen  die Verbrennung der Haul-Ultraschall В Scan Untersuchung Dissertation an der Medizinischen Fakultat der Ludwig Maximilians Universität Munchen

[9] British Standards Institution (BSI): Medical information on human reaction to skin contact with hot surfaces, PD 6504: 1983